**Electric equipment and grounding devices test reports (OPS.03.04.05)**

Installation, setup, testing and operation of electric equipment on well servicing unit shall be conducted in accordance with «Electric Installation Rules», «Power Systems Safety Standards».

Upon completion of well servicing equipment installation, metal works of electric installations, frameworks of electric equipment and drive mechanisms should be earth grounded in accordance with «Electric Installation Rules» to provide safety to people. Before start up and run of equipment technical conditions of grounding devices shall be tested. Such test includes:

* Check of technical condition of grounding devices and electric equipment by specialized electric laboratory upon request of \_\_\_\_\_\_\_\_\_ Company and in accordance with its instructions.
* «Electric equipment and Grounding devices test Report» shall be executed upon results of testing and passed to the well servicing Contractor.
* Documents shall be kept by well servicing foreman.

(Persons in charge: Chief Power Engineer of \_\_\_\_\_\_\_\_\_Company and well servicing Contractor).